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Datasets description
DEM 90m resolution SRTM data of Xinjiang Uygur Autonomous Region 
Data source description
Obtained from the geospatial data cloud (https://www. gscloud. cn/）。SRTM (Shuttle Radar Topography Mission) has undergone multiple revisions, and the current data revision version is V4.1. This version is obtained by CIAT (International Center for Tropical Agriculture) using a new interpolation algorithm to obtain SRTM terrain data. This method better fills the data hole in SRTM90. The interpolation algorithm comes from Reuter et al.（2007） SRTM terrain data can be divided into SRTM1 and SRTM3 according to accuracy, and the corresponding resolution accuracies are 30 meters and 90 meters respectively (currently public data is data with a resolution of 90 meters).
Data processing method

Data quality description
 
Base information
data size:933.7 MiB
data format:Geotiff format
Coordinate system: WGS84 
Projection  
Keywords
Theme:None, None
	Subject:Cartography 
	Time:2023
	Place:None 
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Service information
contacts:None 
phone:0991-7823121
mailbox:datacenter@ms.xjb.ac.cn
Contact information
contributors:shao qian ying 
author:shao qian ying  
manager:zhao jin 
Project information
Citations and annotations
In order to protect the rights and interests of the platform's scientific and technological resources, expand the services of the platform center, and enhance the application potential of scientific and technological resources,resource users are requested to mark and quote the research results (including published papers, treatises, data products, unpublished research reports, data products, etc.) generated by the use of resources in the following manner.
For the achievements published in English, please refer to the following specifications：
The dataset is provided by Arid Land Ecology and Resources Science Data Center(https://data.dcxjegi.cn).
Data reference:
shao qian ying. DEM 90m resolution SRTM data of Xinjiang Uygur Autonomous Region. Arid Land Ecology and Resources Science Data Center(https://data.dcxjegi.cn), 2026. 




